{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":50,"n_cols":5,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
["Wire & Sheet Metal Gage Table",null,null,null,"(Ref : Aircraft Mechanics Digest, Palomar Books)"]
[]
["No of\nGage","American or\nBrown & Shape AWG","Washburn & Moen\nW & MG","Birmingham or\nStub's Iron Wire BWG","U.S. Standard For Plate\nUSG"]
["7-0",null,0.49,null,0.5]
["6-0",0.57999999999999996,0.161,null,0.46800000000000003]
["5-0",0.51600000000000001,0.43,0.5,0.437]
["4-0",0.46,0.39300000000000002,0.45400000000000001,0.40600000000000003]
["3-0",0.40899999999999997,0.36199999999999999,0.42499999999999999,0.375]
["2-0",0.36399999999999999,0.33100000000000002,0.38,0.34300000000000003]
[0,0.32400000000000001,0.30599999999999999,0.34,0.312]
[1,0.28899999999999998,0.28299999999999997,0.3,0.28100000000000003]
[2,0.25700000000000001,0.26200000000000001,0.28399999999999997,0.26500000000000001]
[3,0.22900000000000001,0.24299999999999999,0.25900000000000001,0.25]
[4,0.20399999999999999,0.22500000000000001,0.23799999999999999,0.23400000000000001]
[5,0.18099999999999999,0.20699999999999999,0.22,0.218]
[6,0.16200000000000001,0.192,0.20300000000000001,0.20300000000000001]
[7,0.14399999999999999,0.17699999999999999,0.18,0.187]
[8,0.128,0.16200000000000001,0.16500000000000001,0.17100000000000001]
[9,0.114,0.14799999999999999,0.14799999999999999,0.156]
[10,0.10100000000000001,0.13500000000000001,0.13400000000000001,0.14000000000000001]
[11,0.09,0.12,0.12,0.125]
[12,0.08,0.105,0.109,0.109]
[13,7.1999999999999995E-2,9.0999999999999998E-2,9.5000000000000001E-2,9.2999999999999999E-2]
[14,6.4000000000000001E-2,0.08,8.3000000000000004E-2,7.8E-2]
[15,5.7000000000000002E-2,7.1999999999999995E-2,7.1999999999999995E-2,7.0000000000000007E-2]
[16,0.05,6.2E-2,6.5000000000000002E-2,6.2E-2]
[17,4.4999999999999998E-2,5.3999999999999999E-2,5.8000000000000003E-2,5.6000000000000001E-2]
[18,0.04,4.7E-2,4.9000000000000002E-2,0.05]
[19,3.5000000000000003E-2,4.1000000000000002E-2,4.2000000000000003E-2,4.2999999999999997E-2]
[20,3.2000000000000001E-2,3.4000000000000002E-2,3.5000000000000003E-2,3.6999999999999998E-2]
[21,2.8000000000000001E-2,3.1E-2,3.2000000000000001E-2,3.4000000000000002E-2]
[22,2.5000000000000001E-2,2.8000000000000001E-2,2.8000000000000001E-2,3.1E-2]
[23,2.1999999999999999E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.8000000000000001E-2]
[24,0.02,2.3E-2,2.1999999999999999E-2,2.5000000000000001E-2]
[25,1.7000000000000001E-2,0.02,0.02,2.1000000000000001E-2]
[26,1.4999999999999999E-2,1.7999999999999999E-2,1.7999999999999999E-2,1.7999999999999999E-2]
[27,1.4E-2,1.7000000000000001E-2,1.6E-2,1.7000000000000001E-2]
[28,1.2E-2,1.6E-2,1.4E-2,1.4999999999999999E-2]
[29,1.0999999999999999E-2,1.4999999999999999E-2,1.2999999999999999E-2,1.4E-2]
[30,0.01,1.4E-2,1.2E-2,1.2E-2]
[31,8.0000000000000002E-3,1.2999999999999999E-2,0.01,0.01]
[32,8.0000000000000002E-3,1.2E-2,8.9999999999999993E-3,0.01]
[33,7.0000000000000001E-3,1.0999999999999999E-2,8.0000000000000002E-3,8.9999999999999993E-3]
[34,6.0000000000000001E-3,0.01,7.0000000000000001E-3,8.0000000000000002E-3]
[35,5.0000000000000001E-3,8.9999999999999993E-3,5.0000000000000001E-3,7.0000000000000001E-3]
[36,5.0000000000000001E-3,8.9999999999999993E-3,4.0000000000000001E-3,7.0000000000000001E-3]
[37,4.0000000000000001E-3,8.0000000000000002E-3,null,6.0000000000000001E-3]
[38,4.0000000000000001E-3,8.0000000000000002E-3,null,6.0000000000000001E-3]
[39,3.0000000000000001E-3,7.0000000000000001E-3]
[40,3.0000000000000001E-3,7.0000000000000001E-3]

{"sheet":"Data","index":1,"n_rows":504,"n_cols":3,"rows_kept":504,"cut":false,"hidden":false,"merged":[]}
["*** ACCELERATION"]
[1,"m/s²"]
[100,"cm/s² (=galileo)"]
[{"$f":"A5*12","v":472.44094488188978},"ft/s²"]
[{"$f":"A2/0.0254","v":39.370078740157481},"in/s²"]
[{"$f":"A2*3600^2","v":12960000},"m/h²"]
[{"$f":"A4*3600^2","v":6122834645.6692915},"ft/h²"]
[0.1019716213,"g (std. Grav)"]
["*** ANGLE "]
[1,"° (Deg)"]
[60,"' (min)"]
[3600,"\" (sec)"]
[{"$f":"A10*PI()/180","v":1.7453292519943295E-2},"rad"]
[{"$f":"A10/360","v":2.7777777777777779E-3},"rev"]
["*** AREA"]
[1,"in²"]
[{"$f":"A16/12^2","v":6.9444444444444441E-3},"ft²"]
[{"$f":"A16*0.0254^2","v":6.4515999999999998E-4},"m²"]
[{"$f":"A18*100^2","v":6.4516},"cm²"]
[{"$f":"A19*10^2","v":645.16},"mm²"]
[{"$f":"A18/1000^2","v":6.4515999999999997E-10},"km²"]
[7.7160499999999997E-4,"yd²"]
[2.55076E-5,"rod²"]
[2.4909799999999998E-10,"mile²"]
[6.4516000000000002E-6,"a (are) "]
[6.4515999999999994E-8,"ha (hectare) "]
[6.3768999999999999E-7,"rood "]
[1.5942300000000001E-7,"acre "]
[1.951609E-4,"Pyung(Korean)"]
[7.0257923999999996E-3,"Ja²(Korean)"]
[6.5051482999999996E-7,"Danbo(Korean)"]
[6.5051482999999996E-8,"Jeongbo(Korean)"]
[4.03225E-4,"Tatami(Japanese)"]
["*** ANGULAR VELOCITY"]
[1,"rad/s"]
[{"$f":"A35/2/PI()","v":0.15915494309189535},"rev/s"]
[{"$f":"A36*60","v":9.5492965855137211},"rev/min (+RPM)"]
[{"$f":"A37*60","v":572.95779513082323},"rev/h"]
[{"$f":"A35*180/PI()","v":57.295779513082323},"° (Deg)/s"]
["*** CAPACITANCE"]
[1,"F (farad)"]
[1000000,"µF"]
[1000000000000,"pF"]
[898700000000,"stF"]
[1.0000000000000001E-9,"abF"]
["*** CHARGE"]
[1,"C (coulomb)"]
[0.1,"abC"]
[2998000000,"stC"]
[2.7777800000000001E-4,"A·h"]
[1.0363800000000001E-5,"Faraday"]
["*** CURRENT"]
[1,"A"]
[1000,"mA"]
[1000000,"µA"]
[2998000000,"stA"]
[0.1,"abA"]
["*** DATA STORAGE"]
[1,"bit"]
[0.125,"byte"]
[2.44140625E-4,"block"]
[1.8353788399999999E-10,"CD-ROM"]
[3.125E-2,"double word"]
[1.5625E-2,"quadruple word"]
[6.25E-2,"word"]
[2.4769217409999999E-11,"DVD(1 layer, 1 side)"]
[1.23846087E-11,"DVD(1 layer, 2 side)"]
[1.369592021E-11,"DVD(2 layer, 1 side)"]
[6.8479601070000001E-12,"DVD(2 layer, 2 side)"]
[8.5753644190000006E-8,"floppy disk,3.5\" HD"]
[1.084202172E-19,"exabyte"]
[0.25,"nibble"]
[1.220703125E-4,"kilobyte"]
[1.1920928960000001E-7,"megabyte"]
[1.164153218E-10,"gigabyte"]
[1.1102230250000001E-16,"petabyte"]
[1.136868377E-13,"terabyte"]
[1.2446248140000001E-9,"Zip disk"]
["*** DATA TRANSFER"]
[1,"byte/sec"]
[8.0000000000000002E-8,"ethernet(100B-T)"]
[7.9999999999999996E-7,"ethernet(10B-T)"]
[8.0000000000000005E-9,"ethernet(gigabit)"]
[1.0000000000000001E-9,"gigabyte/sec"]
[1.25E-4,"ISDN(64k)"]
[6.2500000000000001E-5,"ISDN(128k)"]
[1E-3,"kilobyte/sec"]
[9.9999999999999995E-7,"megabyte/sec"]
[2.6666666669999999E-2,"modem(300)"]
[6.6666666670000003E-3,"modem(1200)"]
[3.3333333329999999E-3,"modem(2400)"]
[8.3333333330000002E-4,"modem(9600)"]
[5.5555555560000004E-4,"modem(14.4k)"]
[2.7777777780000002E-4,"modem(28.8k)"]
[2.3809523809999999E-4,"modem(33.6k)"]
[1.428571429E-4,"modem(56k)"]
[5.18134715E-6,"T1"]
[1.267427123E-6,"T2"]
[1.788268956E-7,"T3"]
[2.9178338E-8,"T4"]
["*** DENSITY "]
[1,"kg/m³"]
[1E-3,"kg/l "]
[1E-3,"g/cm³ (g/ml) "]
[1,"g/l"]
[1E-3,"t/m³"]
[3.6127300000000002E-5,"lb/in³"]
[6.2427999999999997E-2,"lb/ft³"]
[1.1228364999999999E-6,"slug/in³"]
[1.9402613999999999E-3,"slug/ft³"]
[8.3453999999999993E-3,"lb/US gal "]
[1.0022400000000001E-2,"lb/UK gal "]
[0.13352600000000001,"oz/US gal "]
[0.160359,"oz/UK gal "]
["*** DIFFUSIVITY"]
[1,"m²/s"]
[10000,"cm²/s"]
[{"$f":"A116/0.0254^2","v":1550.0031000062002},"in²/s"]
[{"$f":"A118/12^2","v":10.763910416709724},"ft²/s"]
[{"$f":"A119*3600","v":38750.077500155006},"ft²/h"]
["*** EMF "]
[1,"V "]
[100000000,"abV"]
[3.3355569999999998E-3,"stV"]
["*** ENERGY/WORK"]
[1,"J (=W·s)"]
[1E-3,"kJ "]
[10000000,"erg "]
[2.777778E-4,"Wh "]
[2.777778E-7,"kWh "]
[2.7777780000000002E-10,"MWh "]
[0.10197199999999999,"kgf·m (kp·m) "]
[10197.200000000001,"gf·cm (p·cm)"]
[0.238846,"cal "]
[2.38846E-4,"kcal "]
[1.35962E-3,"KS·s"]
[3.7767259999999997E-7,"KS·h"]
[6.242E+18,"eV"]
[6242000000000,"MeV"]
[23.730399999999999,"ft·pdl"]
[0.73756200000000005,"lbf·ft"]
[3.7250599999999999E-7,"hp·h"]
[9.47817E-4,"Btu"]
[6702412869,"amu"]
[5.0344800000000001E+22,"wavenumber"]
[9.8689499999999996E-3,"liter·atm"]
["*** ENTHALPY "]
[1,"J/kg (=gray)"]
[1E-3,"kJ/kg "]
[2.38846E-4,"cal/g "]
[0.238846,"cal/kg "]
[2.38846E-4,"kcal/kg "]
[4.2992280000000001E-4,"Btu/lb "]
[1,"sievert"]
[100,"rem"]
["*** ENTROPY "]
[1,"J/kg·°C"]
[1E-3,"kJ/kg·°C"]
[2.38846E-4,"cal/g·°C"]
[0.238846,"cal/kg·°C"]
[2.38846E-4,"kcal/kg·°C"]
[2.38846E-4,"Btu/lb·°F"]
["*** FIELD STRENGTH"]
[1,"V/m"]
[3.3359999999999999E-5,"stV/cm"]
[0.01,"V/cm"]
[2.5399999999999999E-2,"V/in"]
[0.30480000000000002,"V/ft"]
["*** FLOW RATE"]
[1,"m³/s"]
[3600,"m³/h"]
[60000,"l/min"]
[1000,"l/s"]
[1000000,"cm³/s"]
[35.314667,"ft³/s"]
[2118.8800030000002,"CFM (=ft³/min)"]
[15850.33214,"US gal/min"]
[13198.161572000001,"UK gal/min"]
[543439.65052799997,"bbl/d(=barrel oil/d)"]
["*** FORCE/WEIGHT"]
[1,"N"]
[1E-3,"kN (=sthene)"]
[100000,"dyne"]
[7.2330100000000002,"pdl (poundal)"]
[0.22480900000000001,"lbf"]
[101.97162,"gf"]
[0.10197162,"kgf (=kp)"]
[101.97162,"p (pond=gf)"]
[3.59694,"ozf"]
[1.00361E-4,"UK tonf"]
[2.248409E-4,"kip"]
["*** FREQUENCY"]
[1,"rad/s"]
[60,"rad/min"]
[{"$f":"A193/2/PI()","v":0.15915494309189535},"Hz (rev/s)"]
[{"$f":"A195/1000","v":1.5915494309189535E-4},"kHz"]
[{"$f":"A196/1000","v":1.5915494309189535E-7},"MHz"]
[{"$f":"A194/2/PI()","v":9.5492965855137211},"rpm (rev/min)"]
[{"$f":"A195*3600","v":572.95779513082323},"rev/h"]
[{"$f":"A193*180/PI()","v":57.295779513082323},"°/s"]
["*** HEAT CAPACITY"]
[1,"J/°C"]
[1E-3,"kJ/°C"]
[0.238846,"cal/°C"]
[2.38846E-4,"kcal/°C"]
[5.26565E-4,"BTU/°F"]
["*** HEAT FLUX"]
[1,"W/m²"]
[1E-3,"kW/m²"]
[1E-4,"W/cm²"]
[9.9999999999999995E-8,"kW/cm²"]
[0.85984499999999997,"kcal/m²·h"]
[2.3884600000000002E-5,"cal/cm²·s"]
[6.1149300000000001E-7,"Btu/in²·s"]
[8.8054999999999996E-5,"Btu/ft²·s"]
[0.316998,"Btu/ft²·h"]
["*** HEAT TRANS.COEFF."]
[1,"W/m²·°C"]
[1E-3,"kW/m²·°C"]
[1E-4,"W/cm²·°C"]
[0.85984499999999997,"kcal/m²·h·°C"]
[2.3884600000000002E-5,"cal/cm²·s·°C"]
[0.17610999999999999,"Btu/ft²·h·°F"]
["*** INDUCTANCE"]
[1,"abH"]
[1.0000000000000001E-9,"H (henry)"]
[1E-3,"µH"]
[9.9999999999999995E-7,"mH"]
[1.1129999999999999E-21,"stH"]
["*** LENGTH"]
[1,"m"]
[100,"cm"]
[1000,"mm"]
[1000000,"µm"]
[10000000000,"Angstrom (Å)"]
[1E-3,"km"]
[39.370100000000001,"in"]
[3.28084,"ft"]
[1.09361,"yd"]
[0.54680700000000004,"fathom"]
[0.19883899999999999,"rod"]
[4.9709700000000002E-2,"chain"]
[4.9709699999999999E-3,"furlong"]
[6.2137100000000001E-4,"mile"]
[5.3995699999999998E-4,"naut.Mile"]
[5.3961199999999997E-4,"UK naut.mile"]
[1.0582011E-16,"ligth year"]
[3.2425420000000003E-17,"parsec"]
[3.3,"Ja (Korean)"]
[2.5000000000000001E-3,"Ri (Korean)"]
["*** MAGNETIC FLUX"]
[1,"maxwell "]
[1E-8,"Wb (weber) "]
[7.9577480000000006E-2,"unit-pole"]
["*** MAGNETIC FIELD"]
[1,"gauss "]
[1E-4,"T (tesla=Wb/m²) "]
[1000,"milligauss"]
[100000,"gamma"]
["*** MASS"]
[1,"kg"]
[1000,"g"]
[1000000,"mg"]
[20000,"water drops"]
[2.2046199999999998,"lb"]
[6.8521799999999994E-2,"slug"]
[35.274000000000001,"oz"]
[1E-3,"t (ton)"]
[9.8420699999999996E-4,"UK ton"]
[1.10231E-3,"US short ton"]
[6.0226450000000001E+26,"amu"]
[266.666,"Don(Korean)"]
[1.6666000000000001,"Gun(Korean)"]
[0.26666000000000001,"Gwan(Korean)"]
["*** MASS FLOW"]
[1,"kg/s "]
[60,"kg/min"]
[3600,"kg/h "]
[1000,"g/s "]
[1E-3,"t/s "]
[0.06,"t/min "]
[3.6,"t/h "]
[2.2046199999999998,"lb/s "]
[132.27719999999999,"lb/min"]
[7936.64,"lb/h "]
["*** MASS FLUX"]
[1,"kg/m²·s"]
[60,"kg/m²·min"]
[3600,"kg/m²·h"]
[1.4223319999999999E-3,"lb/in²·s"]
[5.1203975000000002,"lb/in²·h"]
[0.2048159,"lb/ft²·s"]
[737.33699999999999,"lb/ft²·h"]
["*** MASS M.O.I."]
[1,"kg·m²"]
[10000,"kg·cm²"]
[10000000,"g·cm²"]
[23.730399999999999,"lb·ft²"]
[3417.17,"lb·in²"]
[54674.8,"oz·in²"]
["*** POTENTIAL/VOLTAGE"]
[1,"V"]
[1E-3,"kV"]
[3.3356499999999999E-3,"stV"]
[1000,"mV"]
[100000000,"abV"]
["*** POWER"]
[1,"W (=J/s=N·m/s)"]
[1E-3,"kW (=kJ/s)"]
[10000000,"erg/s"]
[0.10197199999999999,"kgf·m/s (=kp·m/s)"]
[1.35962E-3,"PS (=KS, metric hp)"]
[0.238846,"cal/s"]
[0.85984499999999997,"kcal/h"]
[1.43307E-2,"kcal/min"]
[5.2656510000000003E-4,"CHU/s"]
[1.8956342399999999,"CHU/h"]
[23.730399999999999,"pdl·ft/s"]
[44.253700000000002,"lbf·ft/min"]
[0.73756200000000005,"lbf·ft/s"]
[1.3410200000000001E-3,"hp"]
[3.41214,"Btu/h"]
[5.6869000000000003E-2,"Btu/min"]
[1.01972E-2,"prony"]
[2.549265E-4,"RT"]
[2.8434499999999998E-4,"US RT (CTR)"]
[2.5900000000000001E-4,"Japan RT"]
["*** PRESSURE/STRESS"]
[1,"Pa (N/m²)"]
[1E-3,"kPa"]
[9.9999999999999995E-7,"Mpa"]
[1.0000000000000001E-9,"Gpa"]
[1E-4,"N/cm²"]
[10,"dyne/cm²"]
[1.0000000000000001E-5,"bar"]
[0.10197199999999999,"kgf/m²(kp/m²) "]
[1.01972E-5,"kgf/cm²(kp/cm²)"]
[0.10197199999999999,"mmAq"]
[4.0146299999999999E-3,"inAq"]
[3.3455300000000002E-4,"ftAq"]
[7.5006200000000004E-3,"mmHg (torr)"]
[7.5006199999999996,"micron"]
[2.9530000000000002E-4,"inHg"]
[9.8692300000000007E-6,"atm"]
[0.67196900000000004,"pdl/ft²"]
[1.45038E-4,"lbf/in²(psi)"]
[2.0885399999999998E-2,"lbf/ft²(psf)"]
[6.4749000000000006E-8,"UK tonf/in²"]
[9.3238500000000005E-6,"UK tonf/ft²"]
["*** RADIATION COEFF."]
[1,"W/m2·K4"]
[1E-3,"KW/m2·K4"]
[1E-3,"W/cm2·K4"]
[0.85984499999999997,"kcal/m2·h·K4"]
[2.3884600000000002E-5,"cal/cm2·s·K4"]
[3.0200000000000001E-2,"Btu/ft2·h·K4"]
["*** RESISTANCE"]
[1,"ab ohm"]
[1.0000000000000001E-9,"ohm"]
[1.1129999999999999E-21,"st ohm"]
["*** SPECIFIC ENERGY"]
[1,"kJ/kg (J/g)"]
[1000,"J/kg"]
[0.24,"cal/g (=kcal/kg)"]
[0.43,"Btu/lb"]
["*** SPECIFIC HEAT"]
[1,"J/kg·°C"]
[1E-3,"kJ/kg·°C"]
[0.238846,"cal/kg·°C"]
[2.38846E-4,"kcal/kg·°C"]
[2.38846E-4,"cal/g·°C"]
[2.38846E-4,"Btu/lb·°F"]
[2.777778E-4,"Wh/kg·°C"]
[2.777778E-7,"kWh/kg·°C"]
["*** SPECIFIC VOLUME "]
[1,"m³/kg"]
[1000,"l/kg"]
[27679.9,"in³/lb"]
[16.0185,"ft³/lb"]
[515.31514500000003,"ft³/slug"]
[35881.4,"ft³/ton"]
[119.8264676,"gal/lb"]
[99.776399999999995,"UK gal/lb"]
["*** SPECIFIC WEIGHT "]
[1,"N/m³",{"$f":"IF(ISNUMBER(#REF!),#REF!/A410,\"\")","v":""}]
[1E-3,"kN/m³",{"$f":"IF(ISNUMBER(#REF!),#REF!/A411,\"\")","v":""}]
[0.1,"dyne/cm³",{"$f":"IF(ISNUMBER(#REF!),#REF!/A412,\"\")","v":""}]
[0.10197199999999999,"kgf/m³",{"$f":"IF(ISNUMBER(#REF!),#REF!/A413,\"\")","v":""}]
[6.3658999999999999E-3,"lbf/ft³",{"$f":"IF(ISNUMBER(#REF!),#REF!/A414,\"\")","v":""}]
["*** SPEED"]
[1,"km/s"]
[1000,"m/s"]
[100000,"cm/s"]
[1000000,"mm/s"]
[3600,"km/h"]
[3600000,"m/h"]
[39370.1,"in/s"]
[3280.84,"ft/s"]
[1093.6099999999999,"yd/s"]
[0.62137100000000001,"mile/s"]
[2362200,"in/min"]
[196850,"ft/min"]
[65616.800000000003,"yd/min"]
[3937010,"yd/h"]
[2236.94,"mile/h (=mph)"]
[1943.84,"knot"]
[1942.6,"UK knot"]
[3.0169552999999998,"Mach @ 0 °C"]
["*** SURF. TENSION",null,{"$f":"IF(ISNUMBER(#REF!),#REF!/A415,\"\")","v":""}]
[1,"lbf/ft"]
[8.3333332999999996E-2,"lbf/in"]
[14.593999999999999,"N/m"]
[1.4881793679999999,"kgf/m"]
[1488.1793680000001,"gf/m"]
[14594,"dyne/cm (mN/m)"]
["*** TEMPERATURE"]
[1,"°C"]
[1,"°F"]
[1,"T"]
[1,"R"]
["*** THERMAL CONDUCT."]
[1,"W/m·°C"]
[1E-3,"kW/m·°C"]
[0.01,"W/cm·°C"]
[1.0000000000000001E-5,"kW/cm·°C"]
[0.85984499999999997,"kcal/h·m·°C"]
[2.3884599999999998E-3,"cal/s·cm·°C"]
[6.9334699999999998,"Btu·in/ft²·h·°F"]
[0.577789,"Btu/ft·h·°F"]
[4.81491E-2,"Btu/in·h·°F"]
["*** TIME"]
[31536000,"sec"]
[525600,"min"]
[8760,"hour"]
[365,"day"]
[52.142856999999999,"week"]
[12,"month"]
[1,"year"]
["*** TORQUE/MOMENT"]
[1,"N·m"]
[10000000,"dyne·cm"]
[0.10197199999999999,"kp·m (kgf·m)"]
[10.1972,"kp·cm (kgf·cm)"]
[23.730399999999999,"pdl·ft"]
[0.73756200000000005,"lbf·ft"]
[8.8507499999999997,"lbf·in"]
[141.61199999999999,"ozf·in"]
[3.2926899999999998E-4,"UK tonf·ft"]
["*** VISCOSITY(DYN.)"]
[1,"Pa·s (N·s/m²)"]
[1,"kg/m·s "]
[10,"P (poise) "]
[1000,"cP (centi poise) "]
[0.10197199999999999,"kgf·s/m²"]
[2.8325400000000002E-5,"kgf·h/m²"]
[0.67196900000000004,"pdl·s/ft²"]
[2.0885399999999998E-2,"lbf·s/ft²"]
[5.8015100000000001E-6,"lbf·h/ft²"]
[0.67114099999999999,"lbm/s·ft"]
["*** VISCOSITY(KIN.)"]
[1,"m²/s"]
[10000,"St (Stokes=cm²/s)"]
[3600,"m²/h"]
[1550,"in²/s"]
[10.7639,"ft²/s"]
[5580010,"in²/h"]
[38750.1,"ft²/h"]
["*** VOLUME"]
[1,"m³"]
[1000,"l "]
[1000000,"cm³ (ml)"]
[1000000000,"mm³ (ul)"]
[20000000,"water drops "]
[61023.744100000004,"in³"]
[35.314700000000002,"ft³"]
[1.3079499999999999,"yd³"]
[28.377600000000001,"bushel "]
[27.496200000000002,"UK bushel "]
[2113.38,"liq pt "]
[1759.76,"UK pt "]
[264.17200000000003,"gal "]
[219.96899999999999,"UK gal "]
[33814,"fl oz "]
[35195.1,"UK fl oz "]
[6.2897999999999996,"bbl (oil) "]
[1056.7,"quart "]
[5543.52,"Hob (Korean)"]
[554.35199999999998,"Doe (Korean)"]
[55.435200000000002,"Mal (Korean)"]
["*** VOLUME FLOW"]
[1,"m³/s"]
[60,"m³/min"]
[3600,"m³/h"]
[1000,"l/s "]
[60000,"l/min"]
[3600000,"l/h"]
[35.314500000000002,"ft³/s"]
[2118.96,"ft³/min"]
[127140,"ft³/h"]
[264.17899999999997,"gal/s "]
[15850.8,"gal/min "]
[951050,"gal/h "]
[30191.9,"bbl/h "]
[724610,"bbl/day "]